# **ABOUT KEYLESS OPEN AND KEYLESS START FOR CADILLAC LYRIQ**

## **Using Keyless Open on Your Cadillac LYRIQ**

**Keyless Unlocking from Driver’s Door:**  
When you approach the vehicle with the key fob within a three-foot range of the door:

1. Press the larger end of the driver’s door handle once to unlock the driver’s door.    
2. Wait for the door to unlatch and open partway.   
3. Grab the handle on the outside door trim and pull open.

**Keyless Unlocking from Passenger Doors:**  
When the doors are locked and the key fob is within three feet of the vehicle’s doors or liftgate:

1. Press the large end of the passenger door handle. This will unlatch the door and unlock all doors.   
2. Once the door has opened partway, grab the handle on the outside door trim and pull open.

If your vehicle is equipped with Keyless Open, it will be enabled upon vehicle delivery. If you don’t want this feature, you can disable it.

Disabling**Keyless Open (not available on all vehicles):**

1. With the vehicle off, press and hold the **Lock**and **Unlock** buttons on the key fob for three seconds.    
2. The turn signal lamps will flash four times to indicate it’s disabled. Now to unlock the vehicle and disarm the alarm system, you will have to press the **Unlock**button on the key fob.

Re-enabling **Keyless Open:**

1. With the vehicle off, press and hold the **Lock**and **Unlock**buttons on the key fob for three seconds.

2. The turn signal lamps will flash two times to indicate **Keyless Open**is enabled.

**Welcome/Walkaway Lighting:**  
When your vehicle detects your key fob within three feet, it will activate Welcome Lighting. Your exterior door handles will light up.     
   
When you turn off and exit the vehicle, the vehicle will activate Walkaway Lighting. You can adjust your entry and exit lighting and more in the vehicle’s Settings menu.

## **General Personalization Settings**

1. Touch **Settings**on the center display.
2. Touch **Vehicle**.
3. Select **Remote Lock**, **Unlock**, **Start**. Here are some features that can be customized:

* **Keyless Open**— Enable/disable
* **Passive Locking**— Automatically locks doors and liftgate after you turn off the vehicle, exit with the key fob and close all the doors
* **Passive Unlocking**— Determine which doors unlock upon the first press of the button on the driver’s door
* **Remote** **Door Unlock**— Changes which doors unlock when you use the key fob Unlock button
* **Remote Left in Vehicle Alert**— Horn chirps if you accidentally leave your key fob in the vehicle after exiting
* **Remote Removed from Vehicle Alert**— Horn chirps if the key fob is removed from the vehicle while it’s still on
* **Remote Unlock Light Feedback** — Exterior lights flash when you unlock the vehicle with the key fob
* **Remote Lock Feedback**— Exterior lights flash and horn sounds when you lock the vehicle with the key fob

## **If the Key Fob Loses Battery or Signal Power**

To unlock your vehicle using the mechanical key inside the key fob:

1. Press the small button on the side of the remote key fob near the bottom. Pull the mechanical key out.   
   NOTE: Never pull the mechanical key out without pressing the button.
2. Locate the key cylinder on the liftgate to the right of the center of the tailgate.
3. Insert the key into the cylinder and turn it to unlock.

To start the vehicle when fob loses power:

1. Inside the vehicle, find the key pocket and place the fob into it. The pocket location varies by vehicle model — check the **Owner’s Manual**.
2. Start the car by pressing the brake pedal and pushing the **Power**button.    
   NOTE: The first time you do this, you’ll see a Driver Information Center (DIC) message indicating no key fob is detected and prompting you to place the fob in the key pocket. When you try again while your key fob is in the key pocket, the vehicle will start.

**ÜBER SCHLÜSSELLOSES ÖFFNEN UND SCHLÜSSELLOSEN START FÜR CADILLAC LYRIQ**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Verwendung des schlüssellosen Öffnens für Ihren Cadillac LYRIQ**

**Schlüsselloses Entriegeln von der Fahrertür aus:**

Wenn Sie sich dem Fahrzeug mit dem Schlüsselanhänger bis auf einen Abstand von einem Meter nähern:

1. Drücken Sie einmal auf das größere Ende des Fahrertürgriffs, um die Fahrertür zu entriegeln.

2. Warten Sie, bis die Tür entriegelt ist und sich ein Stück weit öffnet.

3. Fassen Sie den Griff an der Türaußenverkleidung und ziehen Sie ihn auf.

**Schlüsselloses Entriegeln von den Beifahrertüren:**

Wenn die Türen verriegelt sind und sich der Schlüsselanhänger in einer Entfernung von weniger als einem Meter von den Türen oder der Heckklappe des Fahrzeugs befindet:

1. Drücken Sie auf das große Ende des Beifahrertürgriffs. Dadurch wird die Tür entriegelt und alle Türen werden entriegelt.

2. Sobald sich die Tür ein Stück weit geöffnet hat, fassen Sie den Griff an der Türaußenverkleidung und ziehen Sie ihn auf.

Wenn Ihr Fahrzeug mit Keyless Open ausgestattet ist, ist diese Funktion bei der Auslieferung des Fahrzeugs aktiviert. Wenn Sie diese Funktion nicht wünschen, können Sie sie deaktivieren.

**Deaktivieren von Keyless Open (nicht bei allen Fahrzeugen verfügbar):**

1. Halten Sie bei ausgeschaltetem Fahrzeug die Tasten Verriegeln und Entriegeln auf dem Schlüsselanhänger drei Sekunden lang gedrückt.

2. Die Blinkleuchten blinken viermal, um anzuzeigen, dass die Funktion deaktiviert ist. Um das Fahrzeug zu entriegeln und die Alarmanlage zu deaktivieren, müssen Sie nun die Entriegelungstaste am Schlüsselanhänger drücken.

Erneutes Aktivieren von Keyless Open:

1. Halten Sie bei ausgeschaltetem Fahrzeug die Tasten Verriegeln und Entriegeln am Schlüsselanhänger drei Sekunden lang gedrückt.

2. Die Blinkleuchten blinken zwei Mal, um anzuzeigen, dass Keyless Open aktiviert ist.

**Welcome/Walkaway-Beleuchtung:**

Wenn Ihr Fahrzeug Ihren Schlüsselanhänger in einem Umkreis von drei Metern erkennt, wird die Begrüßungsbeleuchtung aktiviert. Die äußeren Türgriffe leuchten dann auf.

Wenn Sie das Fahrzeug abstellen und verlassen, aktiviert das Fahrzeug die Wegfahrbeleuchtung. Sie können die Ein- und Ausstiegsbeleuchtung und weitere Einstellungen im Einstellungsmenü des Fahrzeugs vornehmen.

**Allgemeine Personalisierungseinstellungen**

1. Berühren Sie Einstellungen auf dem mittleren Display.

2. Berühren Sie Fahrzeug.

3. Wählen Sie Fernverriegelung, Entriegelung, Start. Hier sind einige Funktionen, die angepasst werden können:

- Schlüsselloses Öffnen - Aktivieren/Deaktivieren

- Passive Verriegelung - Verriegelt Türen und Heckklappe automatisch, wenn Sie das Fahrzeug ausschalten, mit dem Schlüsselanhänger aussteigen und alle Türen schließen

- Passive Entriegelung - Legt fest, welche Türen bei der ersten Betätigung der Taste an der Fahrertür entriegelt werden

- Fernentriegelung - Ändert, welche Türen entriegelt werden, wenn Sie die Entriegelungstaste am Schlüsselanhänger betätigen

- Fernbedienungsalarm - Die Hupe ertönt, wenn Sie Ihren Schlüsselanhänger nach dem Aussteigen versehentlich im Fahrzeug zurücklassen

- Alarm bei Fernbedienung aus dem Fahrzeug entfernt - Die Hupe ertönt, wenn der Schlüsselanhänger aus dem Fahrzeug entfernt wird, während es noch eingeschaltet ist.

- Remote Unlock Light Feedback - Die Außenbeleuchtung blinkt, wenn Sie das Fahrzeug mit dem Schlüsselanhänger entriegeln.

- Rückmeldung bei Fernverriegelung - Die Außenbeleuchtung blinkt und die Hupe ertönt, wenn Sie das Fahrzeug mit dem Schlüsselanhänger verriegeln

Wenn die Batterie oder das Signal des Schlüsselanhängers ausfällt